{"text_format":"3","workbook":"xlsb","n_sheets":1,"sheets":["ceník"],"not_rendered":{"images":1},"read":"bin_skipped_in_rows","date_system":"1900","formulas":"cached_only","passed_over":{"ids":[37,38,1024],"n":0}}

{"sheet":"ceník","index":0,"n_rows":55,"n_cols":6,"rows_kept":55,"merged":[[53,1,54,1]],"read":"bin_skipped_in_rows","flags":["formulas_cached_only","records_skipped"],"rows_in_doubt":{"n":0,"rows":[]},"rows_in_doubt_other":1}
[{"$nulls":4},"561 53, Dolní Čermná 208"]
[{"$nulls":4},"Mobil: 605 130 166"]
[{"$nulls":4},"E-mai: stavebniny.cermna@centrum.cz"]
[{"$nulls":4},"IČO: 729 22 095, DIČ: CZ7711013695 "]
[]
[null,"NÁZEV","POPIS","CENA VČ. DPH","CENA BEZ DPH","SPOTŘEBA"]
[null,"MULTIBAT PLUS - 30 kg","univerzální zdící a omítková malta",{"v":100.8,"d":"100.80"},{"v":84,"d":"84.00"},"30 kg = 100 l malty, 8 m2 omítky tl. 15 - 20 mm"]
[null,"CEM II/B-M 32,5R - 25 kg","cement 325",{"v":70.8,"d":"70.80"},{"v":59,"d":"59.00"}]
[null,"Hydrát váp. CL 90 CARMEUSE - 20 kg","hydrát velmi jemný",{"v":75.6,"d":"75.60"},{"v":63,"d":"63.00"}]
[null,"Prince Color Z 301 PR - 20 kg","zdící lepidlo na pórobeton",124.32,{"v":103.6,"d":"103.60"},"20 kg/m3 tvárnic"]
[null,"Prince Color K 01 - 30 kg","univerzální zdící a omítková malta vč. písku",{"v":106.2,"d":"106.20"},{"v":88.5,"d":"88.50"},"16-18 kg při tl. ložné spáry 10 mm"]
[null,"Prince Color K 04 - 30 kg","vnitřní štuk zrnitost 0-0,5 mm",{"v":140.4,"d":"140.40"},{"v":117,"d":"117.00"},"3 kg při tl. 2 mm"]
[null,"Prince Color K 12 - 30 kg","vnitřní štuk zrnitost 0-1 mm",{"v":140.4,"d":"140.40"},{"v":117,"d":"117.00"},"3 kg při tl. 2 mm"]
[null,"Prince Color K 13 - 30 kg","vnější a vnitřní štuk zrnitost 0-1 mm",163.68,{"v":136.4,"d":"136.40"},"4 kg při tl. 3 mm"]
[null,"Prince Color EBF jemný beton - 30 kg","vyrovnávací beton 10-30 mm",{"v":104.75999999999999,"d":"104.76"},{"v":87.3,"d":"87.30"},"18 kg při tl. 10 mm"]
[null,"Prince Color Plastifikátor - 5 l",null,{"v":668.4,"d":"668.40"},{"v":557,"d":"557.00"}]
[null,"Prince Color Multifix PP - 5 kg","blesková fixační malta - vnitřní i vnější - 5 min",{"v":294,"d":"294.00"},{"v":245,"d":"245.00"},"1,75 kg na 1 litr malty"]
[null,"Prince Color NC 510 - 25 kg","samonivelační stěrka 2-10mm",{"v":445.2,"d":"445.20"},{"v":371,"d":"371.00"},"1,7 kg při tl. 1 mm"]
[null,"Prince Color Z 301 K - 25 kg","mrazuvzdor. lepidlo na obklady a dlažby ",{"v":137.4,"d":"137.40"},{"v":114.5,"d":"114.50"},"2,4 - 5 kg dle obkladů (1,4 kg/m2 při tl. 1 mm)"]
[null,"Prince Color Z 301 Speciál - 25 kg","flexibilní lepidlo na obklady a dlažby",{"v":324.59999999999997,"d":"324.60"},{"v":270.5,"d":"270.50"},"2,5 - 6 kg dle obkladů (1,4 kg/m2 při tl. 1 mm)"]
[null,"Prince Color IZOL G - 5 l","asfaltový nátěr - penetrace",{"v":858,"d":"858.00"},{"v":715,"d":"715.00"},"penetrace 0,05 l, dvojtý ochranný nátěr 0,5 l"]
[null,"Prince Color IZOL B - 20 kg","hydroizolační pružná stěrka ",{"v":2736,"d":"2,736.00"},{"v":2280,"d":"2,280.00"},"2,5 kg  při tl. 2 mm"]
[null,"Prince Color IZOL Band šedá - 50 m","koutová izolační páska ",{"v":4020,"d":"4,020.00"},{"v":3350,"d":"3,350.00"}]
[null,"Prince Color IZOL M 100x100 mm","manžeta k utěsnění prostupů",{"v":112.8,"d":"112.80"},{"v":94,"d":"94.00"}]
[null,"Prince Color IZOL M 380x380 mm","manžeta k utěsnění prostupů",{"v":450,"d":"450.00"},{"v":375,"d":"375.00"}]
[null,"Prince Color Multigrund PGM - 20 kg","penetrační nátěr ",{"v":2148,"d":"2,148.00"},{"v":1790,"d":"1,790.00"},"0,1 kg při ředění 1:1"]
[null,"Prince Color Multigrund PGM - 10 kg","penetrační nátěr ",{"v":1140,"d":"1,140.00"},{"v":950,"d":"950.00"},"0,1 kg při ředění 1:1"]
[null,"Prince Color Multigrund PGM - 5 kg","penetrační nátěr ",{"v":612,"d":"612.00"},{"v":510,"d":"510.00"},"0,1 kg při ředění 1:1"]
[null,"Prince Color Multigrund PGM - 1 kg","penetrační nátěr ",{"v":163.2,"d":"163.20"},{"v":136,"d":"136.00"},"0,1 kg při ředění 1:1"]
[null,"Prince Color Z 301 PU EPS - 0,75 lt","nízkoexpanzní pěna pro EPS a XPS",{"v":210,"d":"210.00"},{"v":175,"d":"175.00"}]
[null,"Prince Color Multifix PU - 0,75 lt","polyuretanová pěna trubičková",{"v":135.6,"d":"135.60"},{"v":113,"d":"113.00"}]
[null,"Prince Color Multifix PU GUN - 0,75 lt","polyuretanová pěna pistolová",{"v":147.6,"d":"147.60"},{"v":123,"d":"123.00"}]
[null,"Prince Color FM-FX šedá - 3 kg","flexibilní spárovací hmota",{"v":115.19999999999999,"d":"115.20"},{"v":96,"d":"96.00"},"0,3 - 1,2 kg dle šířky spáry"]
[null,"Prince Color FM-FX bílá - 3 kg","flexibilní spárovací hmota",{"v":129.6,"d":"129.60"},{"v":108,"d":"108.00"},"0,3 - 1,2 kg dle šířky spáry"]
[null,"Prince Color FM-S - 310 ml","neutrální silikonová hmota - barevné",{"v":139.2,"d":"139.20"},{"v":116,"d":"116.00"},"15 bm/balení"]
[null,"Prince Color FM-S - 310 ml","neutrální silikonová hmota - bílá, šedá, transpar",{"v":111.6,"d":"111.60"},{"v":93,"d":"93.00"},"15 bm/balení"]
[null,"Akrylátový tmel 310 ml",null,{"v":57.995999999999995,"d":"58.00"},48.33]
[null,"sádra bílá GYPSTREND - 30 kg",null,{"v":274.8,"d":"274.80"},{"v":229,"d":"229.00"}]
[null,"FILTEK 300 g/m2 - 100 m2","geotextílie",28.92,{"v":24.1,"d":"24.10"}]
[null,"FILTEK 150 g/m2 - 100 m2","geotextílie",{"v":18,"d":"18.00"},{"v":15,"d":"15.00"}]
[null,"VERTEX R131 162 g/m2- 55 m2","perlinka",{"v":24,"d":"24.00"},{"v":20,"d":"20.00"}]
[null,"DEKGLASS G200 S40 (10m2)","izolace - asfaltový pás typu S",{"v":132,"d":"132.00"},{"v":110,"d":"110.00"}]
[null,"PE fólie tl. 0,2 mm - 100 m2",null,12.96,{"v":10.8,"d":"10.80"}]
[null,"DEKDREN N8 š. 1 m - 20 m2","nopová fólie",{"v":58.8,"d":"58.80"},{"v":49,"d":"49.00"}]
[null,"GLYNWED PVC flexi roura 80","drenážní roura s otvory",32.76,{"v":27.3,"d":"27.30"}]
[null,"Páska UV, PVC - 33m","lepící páska š. 50mm PVC",{"v":51.6,"d":"51.60"},{"v":43,"d":"43.00"}]
[null,"Páska papírová PROFI 80°C","lepící páska š. 50mm papírová",{"v":78,"d":"78.00"},{"v":65,"d":"65.00"}]
[{"$nulls":3},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
[{"$nulls":3},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
[{"$nulls":3},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
[{"$nulls":3},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
[{"$nulls":3},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
[]
[null,"OTVÍRACÍ DOBA:","Po - Pá ………………. 8:00 - 11:30, 12:30 - 18:00"]
[null,null,"So …………………….. 9:00 - 11:00"]